[image: D:\Fotos profissional\Tese\DSCF3656.JPG]
Figure 1. Vertical collector used in determining the volumetric distribution uniformity.
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Figure 2. Speed vertical distribution of air at 0.5 m from the outlet of the fan.
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Figure 3. Device used to measure the uniformity of volumetric distribution vertical.
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Figure 4. Uniform volumetric distribution vertical.
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