Table 1. Summary of the analysis of variance for stem height (AC), stem diameter (DC), dry mass of the stem (MSC) and dry mass of leaf (MSF) depending on the different blades irrigation resulting from different evaporation percentage of tank class "A".
	Source of variation
	GL
	Mean square

	
	
	AC (cm)
	DC (mm)
	MSC (kg)
	MSF (kg)

	Blades
	6
	1385.42857*
	15.94478ns
	0.00233ns
	0.03075ns

	Residue
	28
	417.05714
	14.17064
	0.00471
	0.01245

	CV
	(%)
	16.77
	16.43
	48.33
	95.84


(**) Significant effect of 1% and (*) a 5% probability; (s) not significant at the 5% level of probability by F test.
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[bookmark: _GoBack]Figure 1. Height stem of corn BRS catingueiro determined on the basis of irrigation water from different evaporation percentage tank class A.
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